**Background pattern

Description automatically generated**

[CC BY-SA 4.0](https://creativecommons.org/licenses/by-sa/4.0/): Open Source Satellite

Reference: KS-DOC-01350

Date: 8th November 2021

Author: James Bayley

VERSION 01

DRAFT

Mercury GS Manual

Table of Contents

[Table of Figures 1](#_Toc87284568)

[1 Document History 1](#_Toc87284569)

[2 Applicable Documents 1](#_Toc87284570)

[3 References 1](#_Toc87284571)

[4 Mercury GS 2](#_Toc87284572)

[4.1 Introduction 2](#_Toc87284573)

[4.2 Telemetry 2](#_Toc87284574)

[4.2.1 Sending A Telemetry Request 2](#_Toc87284575)

[4.2.2 Sending A Telemetry Request Continuously 3](#_Toc87284576)

[4.2.3 Receiving a Telemetry Response 3](#_Toc87284577)

[4.2.4 Receiving a Telemetry Rejection Response 4](#_Toc87284578)

[4.3 Telecommands 5](#_Toc87284579)

[4.3.1 Sending A Telecommand Request 5](#_Toc87284580)

[4.3.2 Sending the Time 5](#_Toc87284581)

[4.3.3 Receiving a Telecommand Response 6](#_Toc87284582)

[4.4 File Transfer 7](#_Toc87284583)

[4.5 Log 8](#_Toc87284584)

[4.6 Config 9](#_Toc87284585)

[4.7 Test 10](#_Toc87284586)

# Document History

Please see the following record of revisions:

|  |  |  |
| --- | --- | --- |
| Document Revision | Document  Status | Change  Description |
| 01 | DRAFT | Initial Revision |
|  |  |  |

# Applicable Documents

The following references are applicable to this document. The latest version of each document applies.

|  |  |  |
| --- | --- | --- |
| Document Reference | Document Title | Reference in this Document |
| KS-DOC-01104 | OSSAT Mercury GS Specification | [Mercury GS Spec] |

# References

The following references are applicable to this document.

|  |  |  |
| --- | --- | --- |
| Document Reference | Document Title | Reference in this Document |
|  |  |  |

Mercury GS

Introduction

This document aims to inform the reader of how to use the Mercury GS Ground Station Software. Terminology related to the Space Industry shall be used in this document, for further information reference the Glossary and the Readme file of the repository. The software is broken up into tabs, and these shall be described in their own headings.

Mercury GS uses its own communications protocol, and formats frames automatically to be sent over the serial link. This protocol is described in the Mercury GS Spec.

**NOTE: This protocol is not representative of one that would be used in Space. It is a simple protocol suitable for lab testing.**

Telemetry

The below image shows the Telemetry tab of Mercury GS. This tab is used to send Telemetry Requests, receive, and display Telemetry Responses and Telemetry Rejection Responses.

Graphical user interface, text, application, email

Description automatically generated

Sending A Telemetry Request

To send a Telemetry Request follow these steps:

1. Type a channel number into the “Channel #” field.
2. Hit the “Send TLM REQ“ button.

NOTE: You will notice the “TIMEOUTS” value go up after sending a Telemetry Request. This is due to not receiving a response within a set time.  
If you send a Telemetry Response back to Mercury GS, with the same channel number and within the timeout period, then the timeout will not count up.  
The timeout period can be adjusted in the CONFIG tab.

Sending A Telemetry Request Continuously

A Telemetry Request can be sent repeatedly to stress test the connection.  
To send a Telemetry Request continuously, follow these steps:

1. Type a channel number into the “Channel #” field.
2. Click the “Continuous?” button.
3. Hit the “Send TLM REQ“ button.

NOTE: The continuous transmission can be cancelled by unchecking the “Continuous?” button. You can also adjust the speed of the continuous transmission by adjusting the “TC/TLM Rate” field on the CONFIG tab, this can be done on the fly and the transmission speed adjusts accordingly.

Receiving a Telemetry Response

We will also want to receive Telemetry Responses from the spacecraft.   
Unfortunately, we don’t all have satellites lying around. So in lieu of one we shall use a terminal program (the steps required to setup the COM ports and a terminal are described in the repository). Pull open your terminal program, we have used Tera Term, and navigate to the Test Frames folder. Send one of the Telemetry Response files in binary.

Graphical user interface, text, application

Description automatically generated

Once this has been successfully sent and received by Mercury GS, you will see the Telemetry Response show up under the “Telemetry” section.

Graphical user interface, text, application, email

Description automatically generated

Receiving a Telemetry Rejection Response

Graphical user interface, text, application, email

Description automatically generatedSimilarly to a Telemetry Response, we can also receive a Telemetry Rejection Response.  
Use your terminal software to send a Rejection Response. It should display under the “Last Failure” section with the Channel Number and the Reason for the rejection.

Telecommands

As well as receiving and requesting Telemetry from the spacecraft, we will want to command it via Telecommands. See below the Telecommand tab of Mercury GS.

Graphical user interface, text, application, email

Description automatically generated

Sending A Telecommand Request

You can send a Telecommand Request by doing the following:

1. Input the Telecommand Number into the “TC #” field.
2. Select the type of the data in the drop down menu. These can be: String, Float, or Integer.
3. Type the you wish to send in the “Data” field. This is validated depending on the type selected in the previous step.
4. Click the “Send TC REQ” button.

NOTE: Telecommands can also transmit continuously and are also subject to timeouts, like with a Telemetry Request check the box to do so. Continuous Rate and Timeout period can be configured in the CONFIG tab.

Sending the Time

You can transmit a Telecommand Request that specifically sends the time to the Spacecraft. To do this either:

* Press the “Send PC Time“ button.
* Enter a date and time into the fields next to the “Send this Time :” button and then hit the forementioned button.

Receiving a Telecommand Response

We can also receive a response to sending a Telecommand. To do so follow the same steps as 4.2.3 (Receiving A Telemetry Response), but instead of sending a Telemetry Response, send a Telecommand Response.  
This will show under the “Last Response” section.

Graphical user interface, text, application, email

Description automatically generated

File Transfer

The below image shows the File Transfer tab.

Graphical user interface, text, application, email

Description automatically generatedNOTE: This tab is not currently implemented and is placeholder/TBD.

Log

The below image shows the Log tab. Graphical user interface, text, application, email

Description automatically generated

NOTE: This tab is not currently implemented and is placeholder/TBD.

Config

The below image shows the Config tab.

Graphical user interface, text, application, email

Description automatically generated

This tab can be used to adjust parameters of Mercury GS. You can change the Continuous Transmission rate in the “TC/TLM Rate” field. Or change the timeout period in the “TC/TLM Timeout” field.

You can also adjust the baud rate that Mercury GS talks over the serial port with the “Comms baud” drop down menu, as well as change the Com Port used with the “Com Port” drop down menu.

All of these configurations can be changed by uploading a config file. This is done using the “Config file” field. NOTE: This feature is not yet implemented.

Test

We may want to test the capability of the Spacecraft to handle invalid frames. The Test tab is used to do this by creating frames that ignore Mercury’s communications protocol and are just sent directly. This tab is shown below.

Graphical user interface, text, application, email

Description automatically generated

Create your message by filling in the fields with the hexadecimal values of the message you wish to send. And then press the “Transmit” button. All data received back from the Spacecraft within a one second window will be displayed in the “Response” field.

A screenshot of a cell phone

Description automatically generated